// Copyright (c) 2013-2018, XMOS Ltd, All rights reserved

/*
Warnings relating to configuration defines located in this XC source file rather than the devicedefines.h header file in order to avoid multiple warnings being issued when the devicedefines.h header file is included in multiple files.
*/

#include "xua_conf_full.h"

#if XUA_USB_EN

#ifndef DEFAULT_FREQ
#warning DEFAULT_FREQ not defined. Using MIN_FREQ
#endif

#ifndef MIN_FREQ
#warning MIN_FREQ not defined. Using 44100
#endif

#ifndef MAX_FREQ
#warning MAX_FREQ not defined. Using 192000
#endif

#ifdef SPDIF_TX
#ifndef SPDIF_TX_INDEX
#warning SPDIF_TX_INDEX not defined! Using 0
#endif
#endif

#ifndef VENDOR_STR
#warning VENDOR_STR not defined. Using "XMOS"
#endif

#ifndef VENDOR_ID
#warning VENDOR_ID not defined. Using XMOS vendor ID (0x20B1)
#endif

#ifndef PRODUCT_STR_A2
#warning PRODUCT_STR_A2 not defined. Using default XMOS string
#endif

#ifndef PRODUCT_STR_A1
#warning PRODUCT_STR_A1 not defined. Using default XMOS string
#endif

#ifndef BCD_DEVICE
#warning BCD_DEVICE not defined. Using XMOS release version number
#endif

#if (AUDIO_CLASS == 1) || (AUDIO_CLASS_FALLBACK)
#ifndef PID_AUDIO_1
#warning PID_AUDIO_1 not defined. Using 0x0003
#endif
#endif

#ifndef PID_AUDIO_2
#warning PID_AUDIO_2 not defined. Using 0x0002
#endif

#ifndef AUDIO_CLASS
#warning AUDIO_CLASS not defined, using 2
#endif

#ifndef AUDIO_CLASS_FALLBACK
#warning AUDIO_CLASS_FALLBACK not defined, using 0 (i.e. disabled)
#endif

/* Sanity check on FS channel counts */
#if (NUM_USB_CHAN_OUT_FS > NUM_USB_CHAN_OUT)
#error NUM_USB_CHAN_OUT_FS expected to be less than or equal to NUM_USB_CHAN_OUT
#endif

#if (NUM_USB_CHAN_IN_FS > NUM_USB_CHAN_IN)
#error NUM_USB_CHAN_IN_FS expected to be less than or equal to NUM_USB_CHAN_IN
#endif

#endif
