<?xml version="1.0" encoding="UTF-8"?>
<Network xmlns="http://www.xmos.com"
         xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"
         xsi:schemaLocation="http://www.xmos.com http://www.xmos.com">
  <Type>Device</Type>
  <Name>XVF3510 Device</Name>

  <Declarations>
    <Declaration>tileref tile[2]</Declaration>
    <Declaration>tileref usb_tile</Declaration>
  </Declarations>

  <Packages>
    <Package id="0" Type="XS2-UFnA-512-TQ128">
      <Nodes>
        <Node Id="0" InPackageId="0" Type="XS2-L16A-512" SystemFrequency="500MHz" OscillatorSrc="1">
          <Boot>
            <Source Location="bootFlash0"/>
          </Boot>
          <Tile Number="0" Reference="tile[0]">
            <Port Location="XS1_PORT_1B" Name="PORT_SQI_CS_0"/>
            <Port Location="XS1_PORT_1C" Name="PORT_SQI_SCLK_0"/>
            <Port Location="XS1_PORT_4B" Name="PORT_SQI_SIO_0"/>
          </Tile>
          <Tile Number="1" Reference="tile[1]"/>
        </Node>
        <Node Id="1" InPackageId="1" Type="periph:XS1-SU" Reference="usb_tile" Oscillator="24MHz">
        </Node>
      </Nodes>
      <Links>
        <Link Encoding="5wire">
          <LinkEndpoint NodeId="0" Link="8" Delays="52clk,52clk"/>
          <LinkEndpoint NodeId="1" Link="XL0" Delays="1clk,1clk"/>
        </Link>
      </Links>
    </Package>
  </Packages>
  
  <Nodes>
    <Node Id="3" Type="device:" RoutingId="0x8000">
      <Service Id="0" Proto="xscope_host_data(chanend c);">
        <Chanend Identifier="c" end="3"/>
      </Service>
    </Node>
  </Nodes>

  <Links>
    <Link Encoding="2wire" Delays="4,4" Flags="XSCOPE">
      <LinkEndpoint NodeId="0" Link="XL0"/>
      <LinkEndpoint NodeId="3" Chanend="1"/>
    </Link>
  </Links>

  <ExternalDevices>
    <Device NodeId="0" Tile="0" Class="SQIFlash" Name="bootFlash0">
      <Attribute Name="PORT_SQI_CS" Value="PORT_SQI_CS_0"/>
      <Attribute Name="PORT_SQI_SCLK" Value="PORT_SQI_SCLK_0"/>
      <Attribute Name="PORT_SQI_SIO" Value="PORT_SQI_SIO_0"/>
    </Device>
  </ExternalDevices>

  <JTAGChain>
    <JTAGDevice NodeId="0"/>
  </JTAGChain>

</Network>
